|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15) Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| PLENARY MEETING | **Addendum 11 to Document xx-E** |
|  | **31 July 2015** |
|  | **Original: English** |
|  | |
| Asia-Pacific Telecommunity Common Proposals | |
| Proposals for the work of the conference | |
|  | |
| Agenda item 1.11 | |

1.11to consider a primary allocation for the Earth exploration-satellite service (Earth-to-space) in the 7-8 GHz range, in accordance with Resolution **650 (WRC‑12)**;

**Introduction:**

APT Members are supportive of a global primary allocation to the Earth exploration-satellite service (Earth-to-space) in the band 7 190-7 250 MHz .

APT Members are also of the view that the allocated services in this band should be adequately protected from potential interference due to the possible new allocation to the Earth exploration-satellite service (Earth-to-space), in accordance with Resolution 650(WRC-12), and no constraints should be placed on these services.

Accordingly, APT Members agreed a text for a Preliminary APT Common Proposal (PACP) with variation to method A of CPM Report.

**Proposals:**

**Regulatory and procedural considerations**

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations  
(See No. 2.1)

MOD ASP/xxA11/1

**5 570-7 250 MHz**

|  |  |  |
| --- | --- | --- |
| **Allocation to services** | | |
| **Region 1** | **Region 2** | **Region 3** |
| ... | | |
| **7 145-7 190** FIXED  MOBILE  SPACE RESEARCH (deep space) (Earth-to-space)  5.458 MOD 5.459 | | |
| **7 190-7 235** EARTH EXPLORATION-SATELLITE (Earth-to-space) ADD 5.A111 ADD 5.B111  FIXED  MOBILE  SPACE RESEARCH (Earth-to-space) MOD 5.460  5.458 MOD 5.459 | | |
| **7 235-7 250** EARTH EXPLORATION-SATELLITE (Earth-to-space) ADD 5.A111  FIXED  MOBILE  5.458 | | |

MOD ASP/xxA11/2

5.459 *Additional allocation:*in the Russian Federation, the frequency bands 7 100-7 155 MHz and 7 190-7 235 MHz are also allocated to the space operation service (Earth-to-space) on a primary basis, subject to agreement obtained under No. **9.21**. Inthe frequency band 7 190‑7 235 MHz, No. **9.21** with respect to the Earth exploration-satellite service (Earth-to-space) does not apply.     (WRC-15)

**Reasons:** In the frequency band 7 190-7 235 MHz RR No. **9.21** is applied to the space operation service in order to provide protection for the existing radio services and shall not be applied with respect to a new service (the EESS) not to impose new constraints on the existing radio service.

MOD ASP/xxA11/3

5.460 No emissions to spacecraft operating in deep space shall be effected in the frequency band 7 190-7 235 MHz. Geostationary satellites in the space research service operating in the frequency band 7 190-7 235 MHz shall not claim protection from existing and future stations of the fixed and mobile services and No. 5.43Adoes not apply.     (WRC-15)

**Reasons:** Deletion of first sentence as consequential changes. Addition of words “spacecraft operating in” to be more precise.

**ADD ASP/xxA11/4**

**5.A111** The usage of the frequency band 7 190-7 250 MHz by the Earth exploration-satellite service shall be limited to tracking, telemetry and command for the operation of the spacecraft and that Earth exploration-satellite service geostationary satellites in this frequency band, shall not claim protection from existing and future stations of the fixed and mobile services and No. **5.43A** does not apply.     (WRC‑15)

**Reasons:** To provide a new allocation to the EESS (Earth-to-space) in the frequency band 7 190-7 250 MHz. The TT&C function could be implemented by pairing this new allocation with the already existing EESS (space-to-Earth) allocation in the frequency band 8 025-8 400 MHz. It restricts the usage of the frequency band 7 190-7 250 MHz to the operation of the EESS spacecraft, because the aim for the Resolution **650 (WRC-12)** is to obtain a new allocation in the frequency range 7-8 GHz for the TT&C operations and no studies regarding other purpose except for TT&C function have been performed. If there were no restriction, this new allocation might be used for other purposes (e.g. data dissemination).

**ADD ASP/xxA11/5**

**5.B111** Space stations in the Earth exploration-satellite service (Earth-to-space) operating in the geostationary satellite orbit shall not claim protection from emissions from the space research service in the frequency band 7 190-7 235 MHz.     (WRC‑15)

**Reasons:**  No constraints should be placed on the allocated space research service in the frequency band 7 190-7 235 MHz   due to the possible new allocation to the Earth exploration-satellite service (Earth-to-space), in accordance with Resolution 650(WRC-12). (WRC‑15)

SUP ASP/xxA11/6

RESOLUTION 650 (WRC‑12)

Allocation for the Earth exploration-satellite service   
(Earth-to-space) in the 7-8 GHz range

The World Radiocommunication Conference (Geneva, 2012),

**Reasons:** This Resolution is no longer necessary.

MOD ASP/xxA11/7

APPENDIX 7 (REV.WRC‑15)

Methods for the determination of the coordination area around an earth  
station in frequency bands between 100 MHz and 105 GHz

ANNEX 7

System parameters and predetermined coordination distances for determination of the coordination area around an earth station

MOD ASP/xxA11/8

TABLE 7b    (Rev.WRC‑15)

**Parameters required for the determination of coordination distance for a transmitting earth station**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Transmitting space radiocommunication  service designation** | | **Fixed-satellite, mobile-satellite** | **Aero-nautical mobile-satellite (R) service** | **Aero-nautical mobile-satellite (R) service** | **Fixed- satellite** | **Fixed- satellite** | **Fixed- satellite** | **Fixed- satellite** | | **Earth exploration-satellite, space  operation, space  research** | | **Fixed-satellite, mobile-satellite, meteorological- satellite** | | **Fixed- satellite** | | **Fixed- satellite** | | **Fixed- satellite** | **Fixed- satellite 3** | **Fixed- satellite** | **Fixed- satellite 3** |
| Frequency bands (GHz) | | 2.655-2.690 | 5.030-5.091 | 5.030-5.091 | 5.091-5.150 | 5.091-5.150 | 5.725-5.850 | 5.725-7.075 | | 7.100-7.250 5 | | 7.900-8.400 | | 10.7-11.7 | | 12.5-14.8 | | 13.75-14.3 | 15.43-15.65 | 17.7-18.4 | 19.3-19.7 |
| Receiving terrestrial service designations | | Fixed, mobile | Aeronautical radio- navigation | Aeronautical mobile (R) | Aeronautical radio- navigation | Aeronautical mobile (R) | Radiolocation | Fixed, mobile | | Fixed, mobile | | Fixed, mobile | | Fixed, mobile | | Fixed, mobile | | Radiolocation radionavigation (land only) | Aeronautical radionavigation | Fixed, mobile | Fixed, mobile |
| Method to be used | | § 2.1 | § 2.1, § 2.2 | § 2.1, § 2.2 |  |  | § 2.1 | § 2.1 | | § 2.1, § 2.2 | | § 2.1 | | § 2.1 | | § 2.1, § 2.2 | | § 2.1 |  | § 2.1, § 2.2 | § 2.2 |
| Modulation at terrestrial station 1 | | A |  |  |  |  |  | A | N | A | N | A | N | A | N | A | N | − |  | N | N |
| Terrestrial station interference parameters and criteria | *p0* (%) | 0.01 |  |  |  |  |  | 0.01 | 0.005 | 0.01 | 0.005 | 0.01 | 0.005 | 0.01 | 0.005 | 0.01 | 0.005 | 0.01 |  | 0.005 | 0.005 |
| *n* | 2 |  |  |  |  |  | 2 | 2 | 2 | 2 | 2 | 2 | 2 | 2 | 2 | 2 | 1 |  | 2 | 2 |
| *p* (%) | 0.005 |  |  |  |  |  | 0.005 | 0.0025 | 0.005 | 0.0025 | 0.005 | 0.0025 | 0.005 | 0.0025 | 0.005 | 0.0025 | 0.01 |  | 0.0025 | 0.0025 |
| *NL* (dB) | 0 |  |  |  |  |  | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 |  | 0 | 0 |
| *Ms* (dB) | 26 2 |  |  |  |  |  | 33 | 37 | 33 | 37 | 33 | 37 | 33 | 40 | 33 | 40 | 1 |  | 25 | 25 |
| *W* (dB) | 0 |  |  |  |  |  | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 |  | 0 | 0 |
| Terrestrial station parameters | *Gx* (dBi) 4 | 49 2 | 6 | 10 | 6 | 6 |  | 46 | 46 | 46 | 46 | 46 | 46 | 50 | 50 | 52 | 52 | 36 |  | 48 | 48 |
| *Te* (K) | 500 2 |  |  |  |  |  | 750 | 750 | 750 | 750 | 750 | 750 | 1 500 | 1 100 | 1 500 | 1 100 | 2 636 |  | 1 100 | 1 100 |
| Reference bandwidth | *B* (Hz) | 4 × 103 | 150 × 103 | 37.5 × 103 | 150 × 103 | 106 |  | 4 × 103 | 106 | 4 × 103 | 106 | 4 × 103 | 106 | 4 × 103 | 106 | 4 × 103 | 106 | 107 |  | 106 | 106 |
| Permissible interference power | *Pr*( *p*) (dBW) in *B* | −140 | −160 | −157 | −160 | −143 |  | −131 | −103 | −131 | −103 | −131 | −103 | −128 | −98 | −128 | −98 | −131 |  | −113 | −113 |

1 A: analogue modulation; N: digital modulation.

2 The parameters for the terrestrial station associated with transhorizon systems have been used. Line-of-sight radio-relay parameters associated with the frequency band 5 725‑7 075 MHz may also be used to determine a supplementary contour with the exception that *Gx* = 37 dBi.

3 Feeder links of non-geostationary-satellite systems in the mobile‑satellite service.

4 Feeder losses are not included.

5 Actual frequency bands are 7 190-7 250 MHz for the Earth exploration-satellite service, 7 100-7 155 MHz and 7 190-7 235 MHz for the space operation service and 7 145-7 235 MHz for the space research service. (WRC-15)

**Reasons:**

Consequential changes as a result of including the new allocation to the EESS (Earth-to-space) in Appendix7, Table 7b (Parameters required for the determination of coordination distance for a transmitting earth station).

ARTICLE 21

Terrestrial and space services sharing frequency bands above 1 GHz

Section III − Power limits for earth stations

MOD ASP/xxA11/9

TABLE **21-3**     (Rev.WRC‑15)

|  |  |  |
| --- | --- | --- |
| **Frequency band** | | **Services** |
| 2 025-2 110 MHz  5 670-5 725 MHz  5 725-5 755 MHz[[1]](#footnote-1)6 | (for the countries listed in No. **5.454** with respect to the countries listed in Nos. **5.453** and **5.455**)  (for Region 1 with respect to the countries listed in Nos. **5.453** and **5.455**) | Earth-exploration-satellite  Meteorological-satellite  Mobile-satellite  Space operation |
| 5 755-5 850 MHz6 | (for Region 1 with respect to the countries listed in Nos. **5.453**, **5.455** and **5.456**) | Space research |
| 5 850-7 075 MHz |  |  |
| 7 190-7 250 MHz |  |  |
| 7 900-8 400 MHz |  |  |
| 10.7-11.7 GHz6 | (for Region 1) |  |
| 12.5-12.75 GHz6 | (for Region 1 with respect to the countries listed in No. **5.494**) |  |
| 12.7-12.75 GHz6 | (for Region 2) |  |
| 12.75-13.25 GHz |  |  |
| 14.0-14.25 GHz | (with respect to the countries listed in No. **5.505**) |  |
| 14.25-14.3 GHz | (with respect to the countries listed in Nos. **5.505**, **5.508** and **5.509**) |  |
| 14.3-14.4 GHz6 | (for Regions 1 and 3) |  |
| 14.4-14.8 GHz |  |  |
| ... |  |  |

**Reasons:** Consequential changes as a result of considering the new allocation to the Earth exploration-satellite service (Earth-to-space) the 7 190-7 250 MHz frequency band.

1. 6 **21.12.1** The equality of right to operate when a band of frequencies is allocated in different Regions to different services of the same category is established in No. **4.8**. Therefore any limits concerning inter-Regional interference which may appear in ITU-R Recommendations should, as far as practicable, be observed by administrations. [↑](#footnote-ref-1)